#!/usr/bin/env python3
"""
Smart City IoT Simulator — Martinique (14.6°N, 61.2°W)
=======================================================
Publie vers MULTIPLES brokers MQTT + context brokers NGSI-LD.

Brokers MQTT:
  - EMQX:       emqx_emqx_1:1883        (sans auth)
  - Mosquitto:  mainfluxlabs-mosquitto:1883  (bunker/bunker)
  - BunkerM:    bunkerm_bunkerm_1:1900  (TLS, bunker/bunker)
  - OpenRemote: openremote-manager-1:1883 (admin/Digitribe972)

Context Brokers REST:
#  - Orion-LD:   fiware-gis-quickstart-orion-1:1026  (NGSI-LD)
#  - Stellio:    stellio-api-gateway:8080             (NGSI-LD)
  - FROST:      frost_allinone-web-1:8080/FROST-Server/v1.1 (SensorThings)

Streaming Platforms:
  - Pulsar:     smart-city-pulsar:8080  (HTTP REST Producer API)
  - Redpanda:   smart-city-redpanda:8082 (Kafka REST Proxy)

Time-Series DB:
  - InfluxDB v2: smart-city-influxdb:8086 (via influxdb-client)

Variables d'environnement:
  PUBLISH_INTERVAL_SEC : intervalle de publication (défaut: 10s)
  BASE_LAT / BASE_LON  : coordonnées de base (défaut: Fort-de-France)
#  ENABLE_ORION=1       : activer Orion-LD (défaut: 1)
#  ENABLE_STELLIO=1     : activer Stellio (défaut: 1)
  ENABLE_FROST=1       : activer FROST-Server (défaut: 1)
  ENABLE_INFLUX=1      : activer InfluxDB v2 (défaut: 1)
  ENABLE_PULSAR=1      : activer Apache Pulsar (défaut: 1)
  ENABLE_REDPANDA=1    : activer Redpanda Kafka (défaut: 1)
"""

import os, sys, json, time, random, signal, queue, threading, ssl, urllib.parse
import paho.mqtt.client as mqtt
import urllib.request, urllib.error
from datetime import datetime, timezone
from typing import Any

# Prometheus metrics
import prometheus_client
from prometheus_client import Counter, Histogram, Gauge, Info

# InfluxDB support
import influxdb_client
from influxdb_client.client.write_api import SYNCHRONOUS

# =============================================================================
# Configuration des brokers MQTT
# Configuration des brokers MQTT
# Utilise les noms de services Docker par défaut
EMQX_HOST = os.environ.get("EMQX_HOST", "emqx_emqx_1")
EMQX_PORT = int(os.environ.get("EMQX_PORT", "1883"))
MOSQUITTO_HOST = os.environ.get("MOSQUITTO_HOST", "smart-city-mosquitto")
MOSQUITTO_PORT = int(os.environ.get("MOSQUITTO_PORT", "1883"))
BUNKERM_HOST = os.environ.get("BUNKERM_HOST", "bunkerm_bunkerm_1")
BUNKERM_PORT = int(os.environ.get("BUNKERM_PORT", "1900"))

# =============================================================================
# Configuration
# =============================================================================
BASE_LAT    = float(os.environ.get("BASE_LAT", "14.6091"))
BASE_LON    = float(os.environ.get("BASE_LON", "-61.2155"))
INTERVAL    = int(os.environ.get("PUBLISH_INTERVAL_SEC", "1"))  # 1s pour temps réel
#ENABLE_ORION   = os.environ.get("ENABLE_ORION", "1") == "1"
#ENABLE_STELLIO = os.environ.get("ENABLE_STELLIO", "1").lower() in ("1", "true", "yes", "on")
ENABLE_FROST   = os.environ.get("ENABLE_FROST", "1") == "1"
ENABLE_OPENREMOTE = os.environ.get("ENABLE_OPENREMOTE", "1") == "1"
OR_ADMIN_USER = os.environ.get("OR_ADMIN_USER", "admin")
OR_ADMIN_PASS = os.environ.get("OR_ADMIN_PASS", "Digitribe972")
OR_REALM     = os.environ.get("OR_REALM", "smartcity")
OR_TOKEN_REALM = os.environ.get("OR_TOKEN_REALM", "master")  # Realm pour obtention token
#ENABLE_IOT_AGENT = os.environ.get("ENABLE_IOT_AGENT", "1") == "1"
FROST_URL    = os.environ.get("FROST_URL", "http://localhost:8090/FROST-Server/v1.1")  # Exposer frost_http-web-1:8080 -> host:8086

# Pulsar config (HTTP REST — pulsar-admin + producer REST API)
ENABLE_PULSAR = os.environ.get("ENABLE_PULSAR", "1").lower() in ("1", "true", "yes", "on")
PULSAR_HOST   = os.environ.get("PULSAR_HOST", "smart-city-pulsar")
PULSAR_PORT   = int(os.environ.get("PULSAR_PORT", "8080"))
PULSAR_BASE   = f"http://{PULSAR_HOST}:{PULSAR_PORT}"

# Redpanda / Kafka config (REST Proxy HTTP)
ENABLE_REDPANDA = os.environ.get("ENABLE_REDPANDA", "1").lower() in ("1", "true", "yes", "on")
REDPANDA_HOST   = os.environ.get("REDPANDA_HOST", "smart-city-redpanda")
REDPANDA_PORT   = int(os.environ.get("REDPANDA_PORT", "8082"))
REDPANDA_BASE   = f"http://{REDPANDA_HOST}:{REDPANDA_PORT}"

# InfluxDB config
ENABLE_INFLUX  = os.environ.get("ENABLE_INFLUX", "1").lower() in ("1", "true", "yes", "on")
INFLUX_URL    = os.environ.get("INFLUX_URL", "http://smart-city-influxdb:8086")  # InfluxDB v2 sur smartcity-shared
INFLUX_ORG    = os.environ.get("INFLUX_ORG", "digitribe")
INFLUX_BUCKET = os.environ.get("INFLUX_BUCKET", "smartcity")  # Correspond au bucket de Telegraf
INFLUX_TOKEN  = os.environ.get("INFLUX_TOKEN", "my-super-token")

# Prometheus metrics HTTP server
METRICS_PORT = int(os.environ.get("METRICS_PORT", "8001"))

# =============================================================================
# Prometheus Metrics Definitions
# =============================================================================

# --- Info ---
simulator_info = Info(
    "simulator", "Smart City Simulator info"
)
simulator_info.info({
    "version": "1.0.0",
    "python_version": sys.version.split()[0],
    "mqtt_brokers": "emqx,mosquitto,bunkerm",
#    "context_brokers": "orion_ld,stellio,frost",
})

# --- Counters ---
messages_published_total = Counter(
    "simulator_messages_published_total",
    "Total messages published by broker",
    ["broker", "sensor_type"]
)

messages_errors_total = Counter(
    "simulator_messages_errors_total",
    "Total publish errors",
    ["broker", "sensor_type", "error_type"]
)

mqtt_connection_total = Counter(
    "simulator_mqtt_connection_total",
    "MQTT connection attempts",
    ["broker", "status"]  # status: success, failure
)

http_requests_total = Counter(
    "simulator_http_requests_total",
    "HTTP requests to REST APIs",
    ["broker", "method", "status_code"]
)

influx_write_total = Counter(
    "simulator_influx_write_total",
    "InfluxDB write operations",
    ["status"]  # success, error
)

# --- Gauges ---
mqtt_broker_connected = Gauge(
    "simulator_mqtt_broker_connected",
    "MQTT broker connection status (1=connected, 0=disconnected)",
    ["broker"]
)

sensors_total = Gauge(
    "simulator_sensors_total",
    "Total number of sensors by type",
    ["sensor_type"]
)

up = Gauge(
    "simulator_up",
    "Simulator is running (1=yes, 0=no)"
)

# --- Histograms ---
publish_duration = Histogram(
    "simulator_publish_duration_seconds",
    "Time spent publishing a message",
    ["broker"],
    buckets=(0.001, 0.005, 0.01, 0.025, 0.05, 0.1, 0.25, 0.5, 1.0, 2.5)
)

http_request_duration = Histogram(
    "simulator_http_request_duration_seconds",
    "HTTP request latency to REST APIs",
    ["broker", "method"],
    buckets=(0.01, 0.05, 0.1, 0.25, 0.5, 1.0, 2.5, 5.0, 10.0)
)

message_payload_size = Histogram(
    "simulator_message_payload_size_bytes",
    "Message payload size in bytes",
    ["broker"],
    buckets=(64, 128, 256, 512, 1024, 2048, 4096, 8192)
)

# Start Prometheus HTTP server in a background thread
def _start_metrics_server():
    def run():
        prometheus_client.start_http_server(METRICS_PORT)
        print(f"[METRICS] 🚀 Prometheus metrics on :{METRICS_PORT}/metrics")
    t = threading.Thread(target=run, daemon=True)
    t.start()
    return t

# Initialize InfluxDB client
_influx_client = None
_influx_write_api = None
if ENABLE_INFLUX:
    try:
        _influx_client = influxdb_client.InfluxDBClient(url=INFLUX_URL, token=INFLUX_TOKEN, org=INFLUX_ORG)
        _influx_write_api = _influx_client.write_api(write_options=influxdb_client.client.write_api.ASYNCHRONOUS)
        print(f"[INFLUX] ✅ Connected to {INFLUX_URL} (async mode)")
    except Exception as e:
        print(f"[INFLUX] ❌ Connection failed: {e}")

SENSOR_COUNTS = {
    "traffic":    int(os.environ.get("SENSOR_COUNT_traffic",    "3")),
    "airquality": int(os.environ.get("SENSOR_COUNT_airquality", "10")),
    "parking":   int(os.environ.get("SENSOR_COUNT_parking",    "10")),
    "noise":     int(os.environ.get("SENSOR_COUNT_noise",      "1")),
    "weather":   int(os.environ.get("SENSOR_COUNT_weather",    "1")),
    "light":     int(os.environ.get("SENSOR_COUNT_light",      "1")),
}
# Si SENSOR_COUNT est défini, multiplier les counts de façon proportionnelle
_total_default = sum(SENSOR_COUNTS.values())
if "SENSOR_COUNT" in os.environ:
    target = int(os.environ["SENSOR_COUNT"])
    ratio = target / _total_default
    for k in SENSOR_COUNTS:
        SENSOR_COUNTS[k] = max(1, int(SENSOR_COUNTS[k] * ratio))

# =============================================================================
# Localisation des capteurs Martinique — Coordonnées FIXES sur terre ferme
# IMPORTANT : ±0.02° autour de Fort-de-France donne ~2km, or Martinique fait
# ~60km de long — certains points tombent en mer. Solution : coordonnées fixes.
# =============================================================================

# Coordonnées réelles Martinique (terre ferme uniquement)
# Martinique : 14.4°N–14.9°N, -61.23°W–-60.8°W
# Coordonnées GPS exactes depuis les assets OpenRemote (realm master)
# Martinique bounds: lat 14.37–14.88°N, lon 61.0–61.25°W
FIXED_LOCATIONS: dict[str, dict[str, tuple[float, float]]] = {
    "traffic": {
        "Fort-de-France Centre":                  (14.6164, -61.07),
        "Le Lamentin Aéroport":                  (14.6167, -61.0035),
        "Le Robert D110":                  (14.6833, -60.9333),
        "Sainte-Anne Plage":                  (14.4333, -60.9833),
        "Saint-Joseph D1":                  (14.7, -61.05),
        "Trinité Centre":                  (14.7167, -60.9167),
        "Le François D2":                  (14.6833, -60.8333),
        "Ducos Penitencier":                  (14.5833, -61.0667),
        "Schœlcher Morne":                  (14.65, -61.1),
        "Case-Pilote Bourg":                  (14.5167, -61.1167),
    },
    "airquality": {
        "Fort-de-France Lamartine":                  (14.613, -61.0667),
        "Le Lamentin Zac":                  (14.62, -61.0),
        "Le Robert Bourg":                  (14.68, -60.93),
        "Sainte-Anne Village":                  (14.43, -60.98),
        "Saint-Joseph Morne":                  (14.705, -61.04),
        "Trinité Eglise":                  (14.72, -60.91),
        "Le François Bourg":                  (14.68, -60.83),
        "Ducos Centre":                  (14.58, -61.06),
        "Schœlcher Plage":                  (14.655, -61.11),
        "Case-Pilote D1":                  (14.52, -61.12),
    },
    "parking": {
        "Fort-de-France Place Clémenceau":                  (14.615, -61.068),
        "Le Lamentin Centre Commercial":                  (14.618, -61.002),
        "Le Robert Stade":                  (14.685, -60.935),
        "Sainte-Anne Mairie":                  (14.432, -60.985),
        "Saint-Joseph Ecole":                  (14.702, -61.045),
        "Trinité Port":                  (14.715, -60.92),
        "Le François Mairie":                  (14.682, -60.835),
        "Ducos ZI":                  (14.585, -61.055),
        "Schœlcher Bourg":                  (14.652, -61.105),
        "Case-Pilote Stade":                  (14.518, -61.118),
    },
    "noise": {
        "Fort-de-France Théâtre":                  (14.617, -61.069),
        "Le Lamentin Zone Industrielle":                  (14.619, -61.001),
        "Le Robert Bourg":                  (14.681, -60.932),
        "Sainte-Anne Plage":                  (14.434, -60.982),
        "Saint-Joseph Morne":                  (14.703, -61.042),
        "Trinité Centre":                  (14.717, -60.918),
        "Le François Bourg":                  (14.681, -60.832),
        "Ducos Penitencier":                  (14.584, -61.058),
        "Schœlcher Morne":                  (14.651, -61.102),
        "Case-Pilote Village":                  (14.519, -61.115),
    },
    "weather": {
        "Fort-de-France Meteo":                  (14.616, -61.067),
        "Le Lamentin Aéroport":                  (14.617, -61.004),
        "Le Robert Bourg":                  (14.682, -60.934),
        "Sainte-Anne Village":                  (14.431, -60.981),
        "Saint-Joseph Morne":                  (14.704, -61.043),
        "Trinité Eglise":                  (14.718, -60.912),
        "Le François Bourg":                  (14.683, -60.834),
        "Ducos Centre":                  (14.586, -61.057),
        "Schœlcher Plage":                  (14.654, -61.108),
        "Case-Pilote D1":                  (14.521, -61.113),
    },
    "light": {
        "Fort-de-France Place":                  (14.6155, -61.0685),
        "Le Lamentin Rond-point":                  (14.6185, -61.0025),
        "Le Robert D110":                  (14.6835, -60.9335),
        "Sainte-Anne Plage":                  (14.4335, -60.9835),
        "Saint-Joseph D1":                  (14.7005, -61.0505),
        "Trinité Centre":                  (14.7165, -60.9165),
        "Le François D2":                  (14.6835, -60.8335),
        "Ducos Penitencier":                  (14.5835, -61.0665),
        "Schœlcher Morne":                  (14.6505, -61.1005),
        "Case-Pilote Bourg":                  (14.5165, -61.1165),
    },
}

# Ranges par type
SENSOR_RANGES: dict[str, dict] = {
    "traffic":    {"vehicle_count":(10,150),"average_speed_kmh":(10,80),
                   "congestion_level":(0,5),"occupancy_percent":(0,100)},
    "airquality": {"pm25_ugm3":(5,80),"pm10_ugm3":(10,150),"no2_ugm3":(5,60),
                   "o3_ugm3":(20,120),"co_mgm3":(0.1,5.0),
                   "temperature_celsius":(20,35),"humidity_percent":(40,95)},
    "parking":    {"total_spots":(50,500),"available_spots":(0,500),
                   "occupancy_percent":(0,100),"turnover_per_hour":(5,50)},
    "noise":      {"noise_level_db":(40,95),"peak_db":(60,110)},
    "weather":    {"temperature_celsius":(22,34),"humidity_percent":(50,95),
                   "wind_speed_kmh":(0,50),"pressure_hpa":(1005,1025),
                   "rain_mm":(0,20),"uv_index":(0,11)},
    "light":      {"brightness_lux":(0,100000),"power_consumption_w":(0,500)},
}

NOISE_CATEGORIES = ["quiet","moderate","loud","very_loud"]
LIGHT_STATUSES   = ["on","off","dimmed","auto"]

# =============================================================================
# Capteurs déclarés
# =============================================================================
SENSORS: dict[str, dict] = {}
counter = 0
for stype, locs in FIXED_LOCATIONS.items():
    for name, coords in locs.items():
        sid = f"{stype}_{counter:03d}"
        SENSORS[sid] = {"type": stype, "lat": coords[0], "lon": coords[1], "name": name}
        counter += 1

# =============================================================================
## Payload NGSI-LD pour Orion-LD / Stellio
# =============================================================================
# Contextes NGSI-LD : core + Smart Data Models
# https://smartdatamodels.org pour les @context officiels
## Contexte NGSI-LD pur pour Orion-LD (vocabulaires standards uniquement)
## Orion-LD ne peut pas résoudre raw.githubusercontent.com — utiliser uri.etsi.org uniquement
#ORION_CONTEXT = [
#    "https://uri.etsi.org/ngsi-ld/v1/ngsi-ld-core-context.jsonld",
#]

# Mapping sensor type → Smart Data Model type NGSI-LD
SMART_MODEL_MAPPING = {
    "airquality": "AirQualityObserved",
    "traffic":    "TrafficFlowObserved",
    "parking":    "OffStreetParking",
    "noise":       "NoiseLevelObserved",
    "weather":    "WeatherObserved",
    "light":       "Device",
}
FROST_HEADERS = {"Accept": "application/json", "Content-Type": "application/json"}

# Cache FROST : éviter de recréer Thing/Datastream
_frost_cache: dict[str, tuple[str, str]] = {}  # (sid, field) -> (thing_id, ds_id)

## Contexte NGSI-LD pur pour Stellio et Orion-LD (vocabulaires standards uniquement)
## Stellio et Orion-LD embarquent le contexte core NGSI-LD : https://uri.etsi.org/ngsi-ld/
# On n'utilise PAS les vocabulaires smartdatamodels.org distants (inaccessibles depuis les containers)
# Les types d'entité Smart Data Models (AirQualityObserved, etc.) sont reconnus par leur nom
# Les propriétés spécifiques sont stockées telles quelles (vocabulaire libre)
#STELLIO_INLINE_CONTEXT = [
#    "https://uri.etsi.org/ngsi-ld/v1/ngsi-ld-core-context.jsonld",
#]

#def _ngsi_payload(sid: str, sensor: dict, context: list | dict = ORION_CONTEXT, source: str = "simulator", topic: str = "") -> dict:
    """Construit un payload NGSI-LD avec Smart Data Models officiels."""
    stype = sensor["type"]
    model_type = SMART_MODEL_MAPPING.get(stype, "Device")
    now = datetime.now(timezone.utc).isoformat()
    
    # Attributs communs à tous les modèles
    payload = {
        "@context": context,
        "id":          f"urn:ngsi-ld:{model_type}:{sid}",
        "type":        model_type,
        "dateObserved": {"type": "Property", "value": now},
        "location":     {"type": "GeoProperty",
                         "value": {"type": "Point",
                                   "coordinates": [sensor["lon"], sensor["lat"]]}},
        "name":         {"type": "Property", "value": sensor["name"]},
        "batteryLevel": {"type": "Property", "value": random.randint(60, 100)},
        # NOUVEAU: Traçabilité MQTT (Conforme NGSI-LD)
        # "source" est un champ standard NGSI-LD (ETSI)
        # "mqttTopic" est une propriété personnalisée (étendue autorisée)
        "source":       {"type": "Property", "value": source},
        "mqttTopic":    {"type": "Property", "value": topic},
    }
    
    # Attributs spécifiques par type de modèle
    ranges = SENSOR_RANGES.get(stype, {})
    props = {}
    for field, val_range in ranges.items():
        if isinstance(val_range, tuple) and len(val_range) == 2:
            lo, hi = val_range
            if isinstance(lo, (int, float)):
                props[field] = {"type": "Property", "value": round(random.uniform(lo, hi), 1)}
        elif isinstance(val_range, list):
            props[field] = {"type": "Property", "value": random.choice(val_range)}
    
    # Mapping vers les noms d'attributs Smart Data Models
    if stype == "airquality":
        if "pm25_ugm3" in props:       payload["NO2"] = props.pop("pm25_ugm3")  # Simplifié
        if "pm10_ugm3" in props:       payload["PM10"] = props.pop("pm10_ugm3")
        if "no2_ugm3" in props:        payload["NO2"] = props.pop("no2_ugm3")
        if "o3_ugm3" in props:         payload["O3"] = props.pop("o3_ugm3")
        if "co_mgm3" in props:         payload["CO"] = props.pop("co_mgm3")
        if "temperature_celsius" in props: payload["temperature"] = props.pop("temperature_celsius")
        if "humidity_percent" in props: payload["relativeHumidity"] = props.pop("humidity_percent")
    
    elif stype == "traffic":
        if "vehicle_count" in props:     payload["vehicleCount"] = props.pop("vehicle_count")
        if "average_speed_kmh" in props: payload["averageVehicleSpeed"] = props.pop("average_speed_kmh")
        if "congestion_level" in props:  payload["congestion"] = props.pop("congestion_level")
        if "occupancy_percent" in props: payload["occupancy"] = props.pop("occupancy_percent")
    
    elif stype == "parking":
        if "available_spots" in props:   payload["availableSpotNumber"] = props.pop("available_spots")
        if "total_spots" in props:        payload["totalSpotNumber"] = props.pop("total_spots")
        if "occupancy_percent" in props:   payload["occupancy"] = props.pop("occupancy_percent")
        if "turnover_per_hour" in props:  payload["turnover"] = props.pop("turnover_per_hour")
    
    elif stype == "noise":
        if "noise_level_db" in props:     payload["noiseLevel"] = props.pop("noise_level_db")
        if "peak_db" in props:            payload["noisePeak"] = props.pop("peak_db")
        payload["noiseCategory"] = {"type": "Property", "value": random.choice(NOISE_CATEGORIES)}
    
    elif stype == "weather":
        if "temperature_celsius" in props: payload["temperature"] = props.pop("temperature_celsius")
        if "humidity_percent" in props:    payload["relativeHumidity"] = props.pop("humidity_percent")
        if "rain_mm" in props:             payload["rainfall"] = props.pop("rain_mm")
        if "uv_index" in props:            payload["uvIndex"] = props.pop("uv_index")
        if "wind_speed_kmh" in props:     payload["windSpeed"] = props.pop("wind_speed_kmh")
    
    elif stype == "light":
        if "brightness_lux" in props:     payload["illuminance"] = props.pop("brightness_lux")
        if "power_consumption_w" in props: payload["power"] = props.pop("power_consumption_w")
        payload["status"] = {"type": "Property", "value": random.choice(LIGHT_STATUSES)}
    
    return payload

def _frost_payload(sid: str, sensor: dict, source: str = "simulator", topic: str = "") -> dict:
    """Construit un payload SensorThings pour FROST-Server."""
    stype = sensor["type"]
    ranges = SENSOR_RANGES.get(stype, {})
    datastreams = []

    for field, val_range in ranges.items():
        if isinstance(val_range, tuple) and len(val_range) == 2:
            lo, hi = val_range
            if isinstance(lo, (int, float)) and isinstance(hi, (int, float)):
                val = round(random.uniform(lo, hi), 1)
                unit = "http://www.qudt.org/vocab/unit#DegreeCelsius"
                obs_prop = {
                    "name":        f"{field} Observation",
                    "description": f"Observation of {field}",
                    "definition":  unit,
                }
                sensor_data = {
                    "name":        f"Sensor {sid} {field}",
                    "description": f"Sensor {sid} measuring {field}",
                    "encodingType": "http://www.opengis.net/doc/IS/SensorML/2.0",
                    "metadata":    {"unit": unit},
                }
                ds = {
                    "name":             f"Datastream {stype}/{field}",
                    "description":      f"Datastream for {stype} sensor {sid} - {field}",
                    "observationType":  "http://www.opengis.net/def/observationType/OGC-OM/2.0/OM_Measurement",
                    "unitOfMeasurement": {"name": field, "symbol": "", "definition": unit},
                    "Sensor":           sensor_data,
                    "ObservedProperty": obs_prop,
                }
                datastreams.append((field, ds, val))

    thing_payload = {
        "name":        f"Thing_{sid}",
        "description": f"Smart City {stype} sensor in Martinique",
        "properties": {
            "sensorType": stype, 
            "region": "Martinique",
            "source": source,      # Traçabilité
            "mqttTopic": topic     # Traçabilité
        },
    }
    return thing_payload, datastreams

# =============================================================================
# HTTP helper
# =============================================================================
def _http_post(url: str, data: dict, headers: dict, broker: str = "unknown") -> str:
    """POST et retourne 'ok' ou 'created' (ou '' si échec)."""
    try:
        body = json.dumps(data).encode()
        req = urllib.request.Request(url, data=body, headers=headers, method="POST")
        with http_request_duration.labels(broker=broker, method="POST").time():
            try:
                with urllib.request.urlopen(req, timeout=8) as resp:
                    http_requests_total.labels(broker=broker, method="POST", status_code=str(resp.status)).inc()
                    if resp.status == 204:
                        return 'created'  # No Content — succès
                    if resp.status not in (200, 201):
                        return ''
                    # Lire le corps pour extraire l'ID (FROST)
                    try:
                        result = json.loads(resp.read())
                        if '@iot.selfLink' in result:
                            link = result['@iot.selfLink']
                            return link.split('(')[1].rstrip(')')
                        if '@iot.id' in result:
                            return str(result['@iot.id'])
                    except Exception:
                        pass
                    location = resp.headers.get('Location', '')
                    if location:
                        return location.split('(')[1].rstrip(')') if '(' in location else ''
                    return 'created'
            except Exception:
                pass
    except urllib.error.HTTPError as e:
        # Lire le corps de l'erreur pour debug
        try:
            err_body = e.read().decode()[:200]
        except Exception:
            err_body = str(e)
        print(f"  ⚠️  HTTP POST {url} → {e.code}: {err_body}")
        http_requests_total.labels(broker=broker, method="POST", status_code=str(e.code)).inc()
        messages_errors_total.labels(broker=broker, sensor_type="http", error_type="http_error").inc()
        return ''
    except Exception as e:
        http_requests_total.labels(broker=broker, method="POST", status_code="exception").inc()
        messages_errors_total.labels(broker=broker, sensor_type="http", error_type="exception").inc()
        print(f"  ⚠️  HTTP POST {url} → {e}")
        return ''

def _http_put(url: str, data: dict, headers: dict, broker: str = "unknown") -> bool:
    try:
        body = json.dumps(data).encode()
        req = urllib.request.Request(url, data=body, headers=headers, method="PUT")
        with http_request_duration.labels(broker=broker, method="PUT").time():
            with urllib.request.urlopen(req, timeout=5) as resp:
                http_requests_total.labels(broker=broker, method="PUT", status_code=str(resp.status)).inc()
                return resp.status in (200, 204)
    except urllib.error.HTTPError as e:
        http_requests_total.labels(broker=broker, method="PUT", status_code=str(e.code)).inc()
        if e.code == 409:
            return True  # Already exists - that's fine
        messages_errors_total.labels(broker=broker, sensor_type="http", error_type="http_error").inc()
        print(f"  ⚠️  HTTP PUT {url} → {e}")
        return False
    except Exception as e:
        http_requests_total.labels(broker=broker, method="PUT", status_code="exception").inc()
        messages_errors_total.labels(broker=broker, sensor_type="http", error_type="exception").inc()
        print(f"  ⚠️  HTTP PUT {url} → {e}")
        return False

# =============================================================================
# MQTT Client multi-broker
# =============================================================================
class MultiMQTT:
    def __init__(self):
        self.clients: dict[str, mqtt.Client] = {}
        self.ok: dict[str, bool] = {}
        self._lock = threading.Lock()
        self._setup()

    def _mk_client(self, name: str, host: str, port: int,
                   tls: bool = False, user: str = "", pwd: str = "",
                   ws: bool = False, use_v5: bool = False) -> mqtt.Client:
        cid = f"smartcity-sim-{name}-{os.getpid()}"
        protocol = mqtt.MQTTv5 if use_v5 else mqtt.MQTTv311
        c = mqtt.Client(client_id=cid, protocol=protocol)
        if user:
            c.username_pw_set(user, pwd)
        if tls:
            c.tls_set(cert_reqs=ssl.CERT_NONE)
            c.tls_insecure_set(True)
        if ws:
            c.ws_set(b"/mqtt")
        c.on_connect = lambda _c, _, __, rc: self._on_connect(name, rc)
        c.on_disconnect = lambda _c, _, __: self._on_disconnect(name)
        try:
            c.connect(host, port, keepalive=30)
            c.loop_start()
        except Exception as e:
            print(f"[MQTT]   ❌ {name} @ {host}:{port} → {e}")
            self.ok[name] = False
        return c

    def _on_connect(self, name: str, rc: int):
        with self._lock:
            if rc == 0:
                self.ok[name] = True
                mqtt_broker_connected.labels(broker=name).set(1)
                mqtt_connection_total.labels(broker=name, status="success").inc()
                print(f"[MQTT]   ✅ {name} connecté")
            else:
                self.ok[name] = False
                mqtt_broker_connected.labels(broker=name).set(0)
                mqtt_connection_total.labels(broker=name, status="failure").inc()
                print(f"[MQTT]   ❌ {name} rc={rc}")

    def _on_disconnect(self, name: str):
        with self._lock:
            self.ok[name] = False
            mqtt_broker_connected.labels(broker=name).set(0)
            print(f"[MQTT]   ⚠️  {name} déconnecté")

    def _setup(self):
        # Utiliser les variables d'environnement pour les brokers
        brokers = [
            ("emqx",      EMQX_HOST,             EMQX_PORT, False, "",       "", False),
            ("mosquitto", MOSQUITTO_HOST,         MOSQUITTO_PORT, False, "",       "", False),  # Same as emqx
            ("bunkerm",   BUNKERM_HOST,           BUNKERM_PORT, False, "bunker", "bunker", False),
        ]
        print("[MQTT] 🔌 Connexion aux brokers...")
        for name, host, port, tls, user, pwd, use_v5 in brokers:
            c = self._mk_client(name, host, port, tls=tls, user=user, pwd=pwd, use_v5=use_v5)
            self.clients[name] = c
            self.ok[name] = False
        time.sleep(3)  # Attend les connexions

    def publish(self, topic: str, payload: str, sensor_type: str = "unknown") -> dict[str, bool]:
        results = {}
        payload_bytes = len(payload.encode())
        with self._lock:
            for name, client in self.clients.items():
                if self.ok.get(name, False):
                    with publish_duration.labels(broker=name).time():
                        try:
                            r = client.publish(topic, payload, qos=1)
                            success = (r.rc == mqtt.MQTT_ERR_SUCCESS)
                            results[name] = success
                            if success:
                                messages_published_total.labels(broker=name, sensor_type=sensor_type).inc()
                                message_payload_size.labels(broker=name).observe(payload_bytes)
                            else:
                                messages_errors_total.labels(broker=name, sensor_type=sensor_type, error_type="mqtt_rc").inc()
                        except Exception:
                            results[name] = False
                            messages_errors_total.labels(broker=name, sensor_type=sensor_type, error_type="exception").inc()
                else:
                    results[name] = False
        return results

#    def publish_iot_agent(self, sid: str, payload: dict, sensor_type: str = "unknown") -> bool:
#        """Publie sur le topic IoT-Agent (json/smartcity-api-key/{sid}/attrs) via les 3 brokers."""
        topic = f"json/smartcity-api-key/{sid}/attrs"
        msg = json.dumps(payload, ensure_ascii=False)
        payload_bytes = len(msg.encode())
        
        success = False
        # Publier sur les 3 brokers: emqx, mosquitto, bunkerm
        for broker_name in ['emqx', 'mosquitto', 'bunkerm']:
            client_ok = self.clients.get(broker_name) is not None and self.ok.get(broker_name, False)
            print(f"[MQTT-DEBUG] {broker_name}: client_exists={self.clients.get(broker_name) is not None}, ok={self.ok.get(broker_name, False)}")
            if client_ok:
                try:
                    r = self.clients[broker_name].publish(topic, msg, qos=1)
                    if r.rc == mqtt.MQTT_ERR_SUCCESS:
                        success = True
#                        messages_published_total.labels(broker='iot-agent', sensor_type=sensor_type).inc()
#                        message_payload_size.labels(broker='iot-agent').observe(payload_bytes)
                except Exception:
#                    messages_errors_total.labels(broker='iot-agent', sensor_type=sensor_type, error_type="exception").inc()
        return success

    def stop(self):
        for name, c in self.clients.items():
            try:
                c.loop_stop()
                c.disconnect()
            except Exception:
                pass

# =============================================================================
# URLs de base (résolues au démarrage)
# =============================================================================
#ORION_HOST = "localhost"
#ORION_PORT = "2026"
#ORION_URL = f"http://{ORION_HOST}:{ORION_PORT}"
#STELLIO_URL = os.environ.get("STELLIO_URL", "http://localhost:8087")  # Stellio API Gateway (à exposer)
# Configuration OpenRemote (URLs dynamiques)
OR_URL      = os.environ.get("OR_URL", "http://localhost:8080")  # OpenRemote Manager (Traefik)
OR_REALM    = os.environ.get("OR_REALM", "smartcity")  # Default: smartcity
OR_TOKEN_URL = os.environ.get("OR_TOKEN_URL", "http://localhost:8080/auth/realms/{OR_REALM}/protocol/openid-connect/token")
OR_TOKEN_TTL = int(os.environ.get("OR_TOKEN_TTL", "3600"))  # Refresh token every hour
#STELLIO_TENANT = os.environ.get("STELLIO_TENANT", "urn:ngsi-ld:tenant:default")



def publish_bunkerm(sid: str, sensor: dict, values: dict) -> bool:
    """Publie sur BunkerM via HTTP API (port 2000) avec session."""
    import base64, http.cookiejar, urllib.request, json
    from datetime import datetime, timezone

    host = "bunkerm_bunkerm_1:2000"
    login_url = f"http://{host}/login"
    data_url = f"http://{host}/api/sensors/data"

    # 1. Cookie jar pour maintenir la session
    cj = http.cookiejar.CookieJar()
    opener = urllib.request.build_opener(urllib.request.HTTPCookieProcessor(cj))

    # 2. Authentification (Basic) pour obtenir le cookie de session
    creds = base64.b64encode(b"bunker:bunker").decode()
    auth_header = {"Authorization": f"Basic {creds}"}

    try:
        # GET sur /login pour initialiser la session
        req_login = urllib.request.Request(login_url, headers=auth_header)
        opener.open(req_login, timeout=5)
    except Exception as e:
        print(f"  ⚠️  BunkerM login → {e}")
        return False

    # 3. Préparer le payload
    payload = {
        "sensor_id": sid,
        "sensor_type": sensor["type"],
        "timestamp": datetime.now(timezone.utc).isoformat(),
    }
    for k, v in values.items():
        if k not in payload:
            payload[k] = v

    # 4. POST avec le cookie de session
    data = json.dumps(payload).encode()
    req = urllib.request.Request(
        data_url,
        data=data,
        headers={**auth_header, "Content-Type": "application/json"},
        method="POST"
    )
    try:
        with http_request_duration.labels(broker="bunkerm", method="POST").time():
            with opener.open(req, timeout=5) as resp:
                http_requests_total.labels(broker="bunkerm", method="POST", status_code=str(resp.status)).inc()
                messages_published_total.labels(broker="bunkerm", sensor_type=sensor["type"]).inc()
                print(f"  ✅ BunkerM: HTTP {resp.status}")
                return resp.status in (200, 201, 204)
    except Exception as e:
        http_requests_total.labels(broker="bunkerm", method="POST", status_code="exception").inc()
        messages_errors_total.labels(broker="bunkerm", sensor_type=sensor["type"], error_type="exception").inc()
        print(f"  ⚠️  BunkerM POST → {e}")
        return False

def publish_frost(sid: str, sensor: dict, field: str, value: float) -> bool:
    """Crée le Thing (1 par capteur) + Datastreams, puis POST l'Observation."""
    # Cache : {sid: (thing_id, {field: ds_id})}
    if sid in _frost_cache:
        thing_id, ds_map = _frost_cache[sid]
        if field in ds_map:
            ds_id = ds_map[field]
            obs_url = f"{FROST_URL}/Datastreams({ds_id})/Observations"
            obs = {
                "resultTime": datetime.now(timezone.utc).isoformat(),
                "result": value,
                "FeatureOfInterest": {
                    "name": f"Location {sid}",
                    "description": f"Feature of interest for sensor {sid}",
                    "encodingType": "application/vnd.geo+json",
                    "feature": {
                        "type": "Point",
                        "coordinates": [sensor.get("lon", -61.0), sensor.get("lat", 14.6)]
                    }
                }
            }
            if _http_post(obs_url, obs, FROST_HEADERS, broker="frost"):
                print(f"  ✅ FROST Observation {sid}/{field} → OK (cached)")
                return True
            else:
                print(f"  ⚠️  FROST Observation {sid}/{field} → échec")
                return False
    
    # Premier appel pour ce capteur : créer Thing + tous les Datastreams
    # Topic MQTT pour traçabilité
    stype = sensor["type"]
    topic = f"city/sensors/{stype}/{sid}"
    thing_payload, datastreams = _frost_payload(sid, sensor, source="simulator", topic=topic)
    print(f"  📊 FROST: POST Thing {sid}...")
    tid = _http_post(f"{FROST_URL}/Things", thing_payload, FROST_HEADERS, broker="frost")
    if not tid:
        print(f"  ⚠️  FROST Thing {sid} → échec création")
        return False
    print(f"  ✅ FROST Thing {sid} créé (ID: {tid})")
    
    # Créer les Datastreams
    ds_map = {}
    for f, ds, _ in datastreams:
        ds["Thing"] = {"@iot.id": tid}
        print(f"  📊 FROST: POST Datastream {sid}/{f}...")
        ds_id = _http_post(f"{FROST_URL}/Datastreams", ds, FROST_HEADERS, broker="frost")
        if ds_id:
            print(f"  ✅ FROST Datastream {sid}/{f} créé (ID: {ds_id})")
            ds_map[f] = ds_id
        else:
            print(f"  ⚠️  FROST Datastream {sid}/{f} → échec")
    
    _frost_cache[sid] = (tid, ds_map)
    
    # Poster l'observation pour le field actuel
    if field in ds_map:
        ds_id = ds_map[field]
        obs_url = f"{FROST_URL}/Datastreams({ds_id})/Observations"
        obs = {"resultTime": datetime.now(timezone.utc).isoformat(), "result": value}
        if _http_post(obs_url, obs, FROST_HEADERS, broker="frost"):
            print(f"  ✅ FROST Observation {sid}/{field} → OK")
            return True
    return False

# =============================================================================
# OpenRemote REST
# =============================================================================
_or_token_cache = {"token": "", "expires": 0}

def _get_or_token() -> str:
    """Obtain an OpenRemote token via password grant (admin user)."""
    import time, urllib.parse
    if _or_token_cache["token"] and _or_token_cache["expires"] > time.time() + 60:
        return _or_token_cache["token"]
    try:
        # Use password grant with admin user (full rights)
        token_url = f"http://localhost:8080/auth/realms/{OR_REALM}/protocol/openid-connect/token"
        client_id = os.environ.get("OR_CLIENT_ID", "openremote")
        client_secret = os.environ.get("OR_CLIENT_SECRET", "QVTnyObwXdpQ0Vuc60kFSonidK49FiXb")
        data = urllib.parse.urlencode({
            "grant_type": "password",
            "username": os.environ.get("OR_ADMIN_USER", "admin"),
            "password": os.environ.get("OR_ADMIN_PASS", "Digitribe972"),
            "client_id": client_id,
            "client_secret": client_secret
        }).encode()
        req = urllib.request.Request(
            token_url,
            data=data,
            headers={"Content-Type": "application/x-www-form-urlencoded"}
        )
        with urllib.request.urlopen(req, timeout=5) as r:
            token_data = json.loads(r.read().decode())
            _or_token_cache["token"] = token_data["access_token"]
            _or_token_cache["expires"] = time.time() + token_data.get("expires_in", 300) - 60
            return _or_token_cache["token"]
    except Exception as e:
        print(f"  ⚠️  OpenRemote token → {e}")
        return ""

def _or_put(asset_id: str, payload: dict) -> bool:
    """PUT update sur un asset OpenRemote (avec version)."""
    token = _get_or_token()
    if not token:
        return False
    try:
        body = json.dumps(payload).encode()
        url = f"{OR_URL}/api/{OR_REALM}/asset/{asset_id}"
        req = urllib.request.Request(url, data=body,
                                    headers={
                                        "Authorization": f"Bearer {token}",
                                        "Content-Type": "application/json",
                                        "If-Match": str(payload.get("version", 1)),
                                    },
                                    method="PUT")
        with http_request_duration.labels(broker="openremote", method="PUT").time():
            with urllib.request.urlopen(req, timeout=5) as resp:
                http_requests_total.labels(broker="openremote", method="PUT", status_code=str(resp.status)).inc()
                messages_published_total.labels(broker="openremote", sensor_type=payload.get("type", "unknown")).inc()
                return resp.status in (200, 204)
    except urllib.error.HTTPError as e:
        http_requests_total.labels(broker="openremote", method="PUT", status_code=str(e.code)).inc()
        messages_errors_total.labels(broker="openremote", sensor_type=payload.get("type", "unknown"), error_type="http_error").inc()
        print(f"  ⚠️  OR PUT {asset_id} → HTTP {e.code}")
        return False
    except Exception as e:
        http_requests_total.labels(broker="openremote", method="PUT", status_code="exception").inc()
        messages_errors_total.labels(broker="openremote", sensor_type=payload.get("type", "unknown"), error_type="exception").inc()
        print(f"  ⚠️  OR PUT {asset_id} → {e}")
        return False

def publish_openremote(sid: str, sensor: dict, values: dict) -> bool:
    """Met à jour les attributs d'un asset OpenRemote via REST."""
    # Mapping sid → asset ID (créés manuellement dans OR)
    ASSET_MAP = {
        "traffic_000":    "7b5c5670d1b84865ba3ac7",  # Traffic Fort-de-France Centre
        "traffic_001":    "557f6e993b994d3cb81017",  # Traffic Fort-de-France North
        "traffic_002":    "cb81dfd2d2dc4d25adc9c2",  # Traffic Fort-de-France South
        "airquality_000": "a51c982a2d3e451898b978",  # Air Quality Fort-de-France
        "parking_000":    "b8f0df19e0af47b386ebb9",  # Parking Fort-de-France Centre
        "noise_000":      "9035103d1866454fb7e451",   # Noise Fort-de-France Centre
        "weather_000":    "b9de80905ac640f488ab27",   # Weather Lamentin Airport
        "light_000":      "ee7823a41e594851ba202f",   # Light Fort-de-France
    }
    asset_id = ASSET_MAP.get(sid)
    if not asset_id:
        return False
    # Construire les attributs à jour
    now = datetime.now(timezone.utc).isoformat()
    attrs = {
        "timestamp": {"type": "DateTime", "value": now, "timestamp": now},
        "battery_level": {"type": "Number", "value": random.randint(60, 100), "timestamp": now},
    }
    # Mapper les valeurs du payload vers les attributs OR
    field_map = {
        "temperature_celsius": "temperature",
        "humidity_percent": "humidity",
        "noise_level_db": "noiseLevel",
        "pm25_ugm3": "airQuality",
        "vehicle_count": "trafficFlow",
        "available_spots": "parking",
        "brightness_lux": "light",
        "flood": "flood",
    }
    for field, val in values.items():
        attr_name = field_map.get(field, field)
        attrs[attr_name] = {
            "type": "Number",
            "value": val,
            "timestamp": now,
            "unit": "µg/m³" if "ugm3" in field else ("°C" if "celsius" in field else ("%" if "percent" in field or "humidity" in field else ("dB" if "db" in field else ""))),
        }
    payload = {
        "id": asset_id,
        "name": sensor["name"],
        "type": "IOTSensor",
        "realm": OR_REALM,
        "attributes": attrs,
    }
    return _or_put(asset_id, payload)

# =============================================================================
# Pulsar — HTTP REST Producer
# API: POST http://host:8080/admin/v2/persistent/public/default/{topic}/produce
# Payload: {"messages": [{"payload": "<base64>", "properties": {...}}]}
# Topics auto-créés par le premier message (Pulsar standalone)
# =============================================================================
_pulsar_session = None

def _get_pulsar_session():
    global _pulsar_session
    if _pulsar_session is None:
        import urllib.request
        _pulsar_session = urllib.request
    return _pulsar_session

def _init_pulsar() -> bool:
    """Teste la connectivité Pulsar au démarrage."""
    try:
        import urllib.request
        req = urllib.request.Request(f"{PULSAR_BASE}/admin/v2/clusters")
        with urllib.request.urlopen(req, timeout=5) as resp:
            if resp.status == 200:
                print(f"[PULSAR] ✅ Connected to {PULSAR_BASE}")
                return True
    except Exception as e:
        print(f"[PULSAR] ⚠️  Cannot reach {PULSAR_BASE}: {e}")
    return False

def publish_pulsar(sid: str, sensor: dict, payload: dict) -> bool:
    """Publie un message sur Pulsar via le client Python (port binaire 6650)."""
    stype = sensor["type"]
    topic = f"persistent://public/default/smartcity-{stype.replace('-','')}"
    try:
        import pulsar
        with publish_duration.labels(broker="pulsar").time():
            client = pulsar.Client(f"pulsar://{PULSAR_HOST}:6650")
            producer = client.create_producer(topic)
            body = json.dumps(payload, ensure_ascii=False).encode()
            producer.send(body, properties={"sensor_id": sid, "source": "simulator"})
            client.close()
        messages_published_total.labels(broker="pulsar", sensor_type=stype).inc()
        message_payload_size.labels(broker="pulsar").observe(len(body))
        return True
    except Exception as e:
        messages_errors_total.labels(broker="pulsar", sensor_type=stype, error_type="exception").inc()
        print(f"  ⚠️  Pulsar → {e}")
        return False

# =============================================================================
# Redpanda / Kafka — HTTP REST Proxy
# API: POST http://host:8082/topics/{topic}
# Payload: {"records": [{"value": "<base64>"}]}
# Topics auto-créés par le premier message (Redpanda)
# =============================================================================
_redpanda_session = None

def _get_redpanda_session():
    global _redpanda_session
    if _redpanda_session is None:
        import urllib.request
        _redpanda_session = urllib.request
    return _redpanda_session

def _init_redpanda() -> bool:
    """Teste la connectivité Redpanda au démarrage."""
    try:
        import urllib.request
        req = urllib.request.Request(f"{REDPANDA_BASE}/v1/status/alive")
        with urllib.request.urlopen(req, timeout=5) as resp:
            if resp.status == 200:
                print(f"[REDPANDA] ✅ Connected to {REDPANDA_BASE}")
                return True
    except Exception as e:
        print(f"[REDPANDA] ⚠️  Cannot reach {REDPANDA_BASE}: {e}")
    return False

def publish_redpanda(sid: str, sensor: dict, payload: dict) -> bool:
    """Publie un message sur Redpanda/Kafka via le REST Proxy."""
    stype = sensor["type"]
    topic = stype  # air-quality, traffic, weather, parking, noise, light
    try:
        import urllib.request, base64
        body = json.dumps(payload, ensure_ascii=False)
        b64 = base64.b64encode(body.encode()).decode()
        record = {
            "records": [{"value": b64}]
        }
        url = f"{REDPANDA_BASE}/topics/{topic}"
        req = urllib.request.Request(
            url,
            data=json.dumps(record).encode(),
            headers={"Content-Type": "application/vnd.kafka.json.v2+json"},
            method="POST"
        )
        with http_request_duration.labels(broker="redpanda", method="POST").time():
            with urllib.request.urlopen(req, timeout=8) as resp:
                http_requests_total.labels(broker="redpanda", method="POST", status_code=str(resp.status)).inc()
                messages_published_total.labels(broker="redpanda", sensor_type=stype).inc()
                message_payload_size.labels(broker="redpanda").observe(len(body.encode()))
                return resp.status in (200, 201, 204)
    except urllib.error.HTTPError as e:
        http_requests_total.labels(broker="redpanda", method="POST", status_code=str(e.code)).inc()
        messages_errors_total.labels(broker="redpanda", sensor_type=stype, error_type="http_error").inc()
        print(f"  ⚠️  Redpanda → {e.code}")
        return False
    except Exception as e:
        http_requests_total.labels(broker="redpanda", method="POST", status_code="exception").inc()
        messages_errors_total.labels(broker="redpanda", sensor_type=stype, error_type="exception").inc()
        print(f"  ⚠️  Redpanda → {e}")
        return False

def publish_influx(sid: str, sensor: dict, values: dict) -> bool:
    """Write sensor data to InfluxDB (async, non-blocking)."""
    if not _influx_write_api:
        influx_write_total.labels(status="skipped").inc()
        return False
    
    def _write_async():
        try:
            stype = sensor["type"]
            lat = sensor.get("lat", BASE_LAT)
            lon = sensor.get("lon", BASE_LON)
            
            points = []
            for field, value in values.items():
                if isinstance(value, (int, float)):
                    p = influxdb_client.Point(stype)\
                        .tag("sensor_id", sid)\
                        .tag("location", sensor.get("name", sid))\
                        .field(field, float(value))\
                        .field("lat", float(lat))\
                        .field("lon", float(lon))
                    points.append(p)
            
            if points:
                _influx_write_api.write(bucket=INFLUX_BUCKET, record=points)
                influx_write_total.labels(status="success").inc()
                print(f"  📈 InfluxDB: {len(points)} points written")
        except Exception as e:
            influx_write_total.labels(status="error").inc()
            print(f"  ⚠️  InfluxDB → {e}")
    
    # Exécution asynchrone (non-bloquante)
    t = threading.Thread(target=_write_async, daemon=True)
    t.start()
    return True  # Async: on ne peut pas savoir immédiatement

def main():
    print("╔══════════════════════════════════════════════════╗")
    print("║  Smart City Simulator — Martinique               ║")
    print("╚══════════════════════════════════════════════════╝")
    print(f"[CFG] Capteurs: {len(SENSORS)}  |  Intervalle: {INTERVAL}s")
#    print(f"[CFG] Orion-LD: {ENABLE_ORION}  |  Stellio: {ENABLE_STELLIO}  |  FROST: {ENABLE_FROST}")
    print(f"[CFG] InfluxDB: {ENABLE_INFLUX}  |  Pulsar: {ENABLE_PULSAR}  |  Redpanda: {ENABLE_REDPANDA}")

    # --- Démarrer le serveur Prometheus ---
    _start_metrics_server()

    # --- Configurer les gauges ---
    for stype, count in SENSOR_COUNTS.items():
        sensors_total.labels(sensor_type=stype).set(count)
    up.set(1)

    # Init connectivity checks
    if ENABLE_PULSAR:
        _init_pulsar()
        # Test immédiat
        print(f"  🌪️ DEBUG: Test Pulsar direct...", flush=True)
        test_payload = {"type": "test", "value": 123}
        test_result = publish_pulsar("test_001", {"type": "air-quality"}, test_payload)
        print(f"  🌪️ DEBUG: Test Pulsar result: {test_result}", flush=True)
    if ENABLE_REDPANDA:
        _init_redpanda()

    mqtt_client = MultiMQTT()

    running = True
    def signal_handler(*_):
        nonlocal running
        running = False
        up.set(0)
        print("\n[SIM] 🛑 Arrêt...")
    signal.signal(signal.SIGINT, signal_handler)
    signal.signal(signal.SIGTERM, signal_handler)

    iteration = 0
    while running:
        iteration += 1
        ts = datetime.now().strftime("%H:%M:%S")
        print(f"\n[SIM] ⏱️  It #{iteration} — {ts}")

        for sid, sensor in SENSORS.items():
            stype = sensor["type"]
            topic = f"city/sensors/{stype}/{sid}"

            # --- Payload MQTT (ATTRIBUTES ONLY - pas de id/type/lat/lon !)
#            # L'IoT Agent n'attend que les readings, pas le body complet
            ranges = SENSOR_RANGES.get(stype, {})
            payload_mqtt = {
                "timestamp": datetime.now(timezone.utc).isoformat(),
                "battery_level": random.randint(60, 100),
            }
            for field, val_range in ranges.items():
                if isinstance(val_range, tuple) and len(val_range) == 2:
                    lo, hi = val_range
                    if isinstance(lo, (int, float)):
                        payload_mqtt[field] = round(random.uniform(lo, hi), 1)
                elif isinstance(val_range, list):
                    payload_mqtt[field] = random.choice(val_range)

            msg = json.dumps(payload_mqtt, ensure_ascii=False)

            # --- MQTT publish ---
            results = mqtt_client.publish(topic, msg, sensor_type=stype)
            ok_mqtt = [n for n, r in results.items() if r]
            if ok_mqtt:
                print(f"  📤 {topic} → {','.join(ok_mqtt)}")

#            # --- IoT-Agent (via EMQX) ---
#            if ENABLE_IOT_AGENT:
#                ok_iot = mqtt_client.publish_iot_agent(sid, payload_mqtt, sensor_type=stype)
#                print(f"  🤖 IoT-Agent: {'✅' if ok_iot else '❌'}")

            # Extraire les valeurs pour OpenRemote
            or_values = {}
            for field, val_range in ranges.items():
                if isinstance(val_range, tuple) and len(val_range) == 2:
                    lo, hi = val_range
                    if isinstance(lo, (int, float)):
                        or_values[field] = round(random.uniform(lo, hi), 1)

            # --- OpenRemote REST ---
            if ENABLE_OPENREMOTE:
                ok_or = publish_openremote(sid, sensor, or_values)
                print(f"  🏠 OpenRemote: {'✅' if ok_or else '⚠️ skipped'}")

#            # --- Orion-LD --- (DÉSACTIVÉ: tout passe par les IoT-Agents MQTT)
#            # if ENABLE_ORION:
#            #     ok_or = publish_orion(sid, sensor)
#            #     print(f"  🌐 Orion-LD: {'✅' if ok_or else '⚠️ skipped'}")

#            # --- Stellio --- (DÉSACTIVÉ: tout passe par les IoT-Agents MQTT)
#            # if ENABLE_STELLIO:
#            #     ok_st = publish_stellio(sid, sensor)
#            #     print(f"  🏢 Stellio:   {'✅' if ok_st else '❌'}")

            # --- FROST ---
            if ENABLE_FROST:
                ranges2 = SENSOR_RANGES.get(stype, {})
                for field, val_range in ranges2.items():
                    if isinstance(val_range, tuple) and len(val_range) == 2:
                        lo, hi = val_range
                        if isinstance(lo, (int, float)):
                            val = round(random.uniform(lo, hi), 1)
                            ok_fr = publish_frost(sid, sensor, field, val)
                            print(f"  📊 FROST:    {'✅' if ok_fr else '❌'}")
    
            # --- InfluxDB ---
            if ENABLE_INFLUX:
                influx_vals = {}
                for field, val_range in ranges.items():
                    if isinstance(val_range, tuple) and len(val_range) == 2:
                        lo, hi = val_range
                        if isinstance(lo, (int, float)):
                            influx_vals[field] = round(random.uniform(lo, hi), 1)
                ok_influx = publish_influx(sid, sensor, influx_vals)
                print(f"  📈 InfluxDB: {'✅' if ok_influx else '❌'}")

            # --- Pulsar (HTTP REST) ---
            if ENABLE_PULSAR:
                print(f"  🌪️ DEBUG: calling publish_pulsar for {sid}, payload_mqtt exists: {bool(locals().get('payload_mqtt'))}", flush=True)
                ok_pulsar = publish_pulsar(sid, sensor, payload_mqtt)
                print(f"  🌪️  Pulsar:  {'✅' if ok_pulsar else '❌'}")

            # --- Redpanda (Kafka REST Proxy) ---
            if ENABLE_REDPANDA:
                ok_redpanda = publish_redpanda(sid, sensor, payload_mqtt)
                print(f"  🐟 Redpanda: {'✅' if ok_redpanda else '❌'}")

            # --- BunkerM HTTP ---
            if os.getenv("BUNKERM_HTTP", "0") == "1":
                ok_bunkerm = publish_bunkerm(sid, sensor, payload_mqtt)
                print(f"  📦 BunkerM:  {'✅' if ok_bunkerm else '❌'}")

        print(f"[SIM]   ✅ {len(SENSORS)} capteurs | MQTT OK: {sum(mqtt_client.ok.values())}/{len(mqtt_client.clients)} | OR: {ENABLE_OPENREMOTE}")

        try:
            time.sleep(INTERVAL)
        except KeyboardInterrupt:
            break

    mqtt_client.stop()
    print("[SIM] ✅ Arrêté proprement.")

if __name__ == "__main__":
    main()
